**General Safety Rules and Code of Conduct**

**(These rules are to be read in conjunction with the specific club rules)**

* 1. Each person is responsible for his/her own and the safety of others, when operating a radio controlled device.
  2. Radio control models are not toys and will be operated responsibly
  3. You will observe the frequency restrictions and controls
  4. You will not start your model un-assisted either by another person or restrained from any movement
  5. You will not power up your model anywhere but in the startup area
  6. You will avoid prop wash over other models, spectators and vehicles
  7. You will do all preflight checks including range checks before you approach the runway
  8. You will call your runway of choice and direction of take off to other pilots
  9. You will observe calls of **Landing**, **Take off**, **Dead stick** and **Low pass or High speed pass** before you approach any runway
  10. You will confirm the flight pattern with the safety officer
  11. You will call Take off before you power up on the runway and wait for confirmation from the other pilots
  12. You will leave the run way as soon as you have achieved adequate altitude
  13. You will not fly over NO fly Zones such as the pits, club house or over parked vehicles
  14. You will fly responsibly and take cognizance of other pilots
  15. You will call low fly and wait for confirmation from other Pilots
  16. On losing power you will call **DEAD STICK**
  17. On landing you will call landing, runway and direction and wait for confirmation
  18. You may taxi to the line before the start up area at which time you will power off.
  19. At any time when you feel that your model may become uncontrollable you will call the situation
  20. You will have responsible fun!